{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":46,"n_cols":6,"rows_kept":46,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXM-M"]
[]
[]
[]
[]
["","","","","","CTXM15M2V1B"]
["Niveau de pression sonore","Chauffage","","Niveau de pression sonore-=-Chauffage-=-Nom.-=-dBA @.","dBA","34"]
["Ventilateur","Débit d'air","Chauffage","Nom.","m³/min","8.7"]
["Niveau de pression sonore","Rafraîchissement","","Nom.","dBA","33"]
["Ventilateur","Débit d'air","Rafraîchissement","Nom.","m³/min","7.9"]
["Caisson","Couleur","","","","Blanc"]
["Dimensions","Unité","","Hauteur","mm","294"]
["","","","Largeur","mm","811"]
["","","","Profondeur","mm","272"]
["Poids","Unité","","","kg","10"]
["Ventilateur","Débit d'air","Rafraîchissement","Haut","m³/min","11.1"]
["","","","Bas","m³/min","6.0"]
["","","","Faible niveau sonore de fonctionnement","m³/min","4.4"]
["","","Chauffage","Haut","m³/min","10.4"]
["","","","Bas","m³/min","6.5"]
["","","","Faible niveau sonore de fonctionnement","m³/min","5.3"]
["Niveau de puissance sonore","Rafraîchissement","","","dBA","57"]
["","Chauffage","","","dBA","54"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","41"]
["","","","Bas","dBA","25"]
["","","","Faible niveau sonore de fonctionnement","dBA","19"]
["","Chauffage","","Haut","dBA","39"]
["","","","Bas","dBA","26"]
["","","","Faible niveau sonore de fonctionnement","dBA","20"]
["Raccords de tuyauterie","Liquide","","DE","mm","6.35"]
["Raccords de tuyauterie","Gaz","","DE","mm","9.5"]
["Raccords de tuyauterie","Évacuation","","","","18"]
["Systèmes de contrôle","Infrared remote control","","","","ARC466A33"]
["","Wired remote control","","","","BRC944B2, BRC073A1"]
["Accessoires standard","Installation manual","","","","1"]
["","AAA dry-cell batteries","","","","2"]
["","Operation manual","","","","1"]
["","Indoor unit fixing screws","","","","2"]
["","Infrared remote control","","","","1"]
["","Mounting plate","","","","1"]
["","Remote control holder","","","","1"]
["","Titanium apatite photocatalytic air purification filter","","","","1"]
["Alimentation électrique","Nom","","","","V1"]
["","Phase","","","","1~"]
["","Fréquence","","","Hz","50"]
["","Alimentation électrique-=-Tension-=-V","","","Vca","220-240"]