{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":6,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKSV-P"]
[]
[]
[]
[]
["","","","","EKSV21P1","EKSV26P1"]
["Montage","","","","Vertical","Vertical"]
["Dimensions","Unité","Hauteur","mm","2000","2000"]
["","","Largeur","mm","1006","1300"]
["","","Profondeur","mm","85","85"]
["Poids","Unité","","kg","35","42"]
["Volume","L","","","1.3","1.7"]
["Surface","Extérieure","","m²","2.01","2.60"]
["","Ouverture","","m²","1.800","2.360"]
["","Absorbeur","","m²","1.80","2.36"]
["Revêtement","","","","Microtherm (absorption max. 96%, Emission env. 5% +/-2%)","Microtherm (absorption max. 96%, Emission env. 5% +/-2%)"]
["Absorbeur","","","","Registre à tubes en cuivre en forme de harpe avec plaque d'aluminium soudée au laser et à revêtement hautement sélectif","Registre à tubes en cuivre en forme de harpe avec plaque d'aluminium soudée au laser et à revêtement hautement sélectif"]
["Couverture transparente","","","","Verre Sécurit, transmission + / - 92 %","Verre Sécurit, transmission + / - 92 %"]
["Angle de toiture autorisé","Min.","","°","15","15"]
["","Max.","","°","80","80"]
["Pression de service","Max.","","bars","6","6"]
["Température à l'arrêt","Max.","","°C","192","192"]
["Performances thermiques","Coefficient de perte thermique a1","","W/m².K²","4.300","4.300"]
["","Température liée au coefficient de perte thermique a2","","W/m².K²","0.006","0.006"]
["Performances thermiques","Puissance calorifique","","kJ/K","4.9","6.5"]