{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":5,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAHG-F / RZAG-LV1"]
[]
[]
[]
[]
["","","","","FCAHG71FVEB / RZAG71L7V1B"]
["Puissance frigorifique","Nom.","","kW","6.8"]
["Puissance calorifique","Nom.","","kW","7.5"]
["Efficacité nominale","EER","","","4.09"]
["","COP","","","4.80"]
["Efficacité nominale","Consommation énergétique annuelle","","kWh","830"]
["Efficacité nominale","Directive sur l'étiquetage énergétique","Rafraîchissement","","A"]
["","","Chauffage","","A"]
["Rafraîchissement des locaux","Classe d’efficacité énergétique","","","A++"]
["","Puissance","Pdesign","kW","6.80"]
["","SEER","","","7.35"]
["","Consommation d’énergie annuelle","","kWh/a","324"]
["Chauffage des locaux (climat tempéré)","Classe d’efficacité énergétique","","","A+"]
["","Puissance","Pdesign","kW","5.65"]
["","SCOP/A","","","4.54"]
["","Pdh Puissance calorifique à -10°","","kW","5.45"]
["","Consommation d’énergie annuelle","","kWh/a","1743"]
["Remarques","","","","(2) - SEER and SCOP are according to EN 14825"]