{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":59,"n_cols":6,"rows_kept":59,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAHG-F"]
[]
[]
[]
[]
["","","","","","FCAHG71FVEB"]
["Caisson","Matériau","","","","Tôle en acier galvanisé"]
["Dimensions","Unité","","Hauteur","mm","288"]
["","","","Largeur","mm","840"]
["","","","Profondeur","mm","840"]
["Poids","Unité","","","kg","25.0"]
["Ventilateur","Débit d'air","Rafraîchissement","Haut","m³/min","21.2"]
["Ventilateur","Débit d'air","Rafraîchissement","Moyen","m³/min","16.7"]
["Ventilateur","Débit d'air","Rafraîchissement","Bas","m³/min","12.2"]
["","","Chauffage","Haut","m³/min","21.2"]
["Ventilateur","Débit d'air","Chauffage","Moyen","m³/min","16.7"]
["Ventilateur","Débit d'air","Chauffage","Bas","m³/min","12.2"]
["Niveau de puissance sonore","Rafraîchissement","","","dBA","53"]
["","Chauffage","","","dBA","53"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","36"]
["Niveau de pression sonore","Rafraîchissement","","Moyen","dBA","33"]
["Niveau de pression sonore","Rafraîchissement","","Bas","dBA","29"]
["","Chauffage","","Haut","dBA","36"]
["","","","Moyen","dBA","33"]
["","","","Bas","dBA","29"]
["Réfrigérant","PRP","","","","675"]
["Raccords de tuyauterie","Liquide","","DE","mm","9.52"]
["Raccords de tuyauterie","Gaz","","DE","mm","15.9"]
["Raccords de tuyauterie","Évacuation","","","","VP25 (I.D. 25/O.D. 32)"]
["Panneau décoratif","Modèle","","","","BYCQ140D7GFW1 - panneau autonettoyant à filtre à mailles fines"]
["","Couleur","","","","Blanc pur (RAL 9010)"]
["","Dimensions","","Hauteur","mm","130"]
["","","","Largeur","mm","950"]
["","","","Profondeur","mm","950"]
["Façade","Façade-=-Poids-=-kg","","","kg","10"]
["Panneau décoratif 2","Panneau décoratif 2-=-Modèle","","","","BYCQ140D7GW1 - Panneau auto-nettoyant"]
["Façade 2","Façade 2-=-Couleur","","","","Blanc pur (RAL 9010)"]
["","Façade 2-=-Dimensions","","Façade 2-=-Dimensions-=-Hauteur-=-mm","mm","130"]
["","","","Façade 2-=-Dimensions-=-Largeur-=-mm","mm","950"]
["","","","Façade 2-=-Dimensions-=-Profondeur-=-mm","mm","950"]
["","Façade 2-=-Poids-=-kg","","","kg","10.3"]
["Panneau décoratif 3","Panneau décoratif 3-=-Modèle","","","","BYCQ140D7W1W - Totalement blanc, Voir remarque 1"]
["Façade 3","Façade 3-=-Couleur","","","","Blanc pur (RAL 9010)"]
["","Façade 3-=-Dimensions","","Façade 3-=-Dimensions-=-Hauteur-=-mm","mm","50"]
["","","","Façade 3-=-Dimensions-=-Largeur-=-mm","mm","950"]
["","","","Façade 3-=-Dimensions-=-Profondeur-=-mm","mm","950"]
["","Façade 3-=-Poids-=-kg","","","kg","5.4"]
["Façade 4","Façade 4-=-Modèle","","","","BYCQ140D7W1 - Blanc avec déflecteurs gris"]
["","Façade 4-=-Couleur","","","","Blanc pur (RAL 9010)"]
["","Façade 4-=-Dimensions","","Façade 4-=-Dimensions-=-Hauteur-=-mm","mm","50"]
["","","","Façade 4-=-Dimensions-=-Largeur-=-mm","mm","950"]
["","","","Façade 4-=-Dimensions-=-Profondeur-=-mm","mm","950"]
["","Façade 4-=-Poids-=-kg","","","kg","5.4"]
["Accessoires standard","Installation manual","","","","Installation manual"]
["","Installation and operation manual","","","","Installation and operation manual"]
["Alimentation électrique","Nom","","","","VE"]
["","Phase","","","","1~"]
["","Alimentation électrique-=-Fréquence","","Fréquence","","50/60"]
["","Alimentation électrique-=-Tension","","Alimentation électrique-=-Tension-=-V","","220-240"]