{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":99,"n_cols":7,"rows_kept":99,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-MS"]
[]
[]
[]
[]
["","","","","","FTXJ50MV1BS","FTXJ20MV1BS (Archived)"]
["Niveau de pression sonore","Chauffage","","Haut","dBA","47"]
["","","","Moyen","dBA","41"]
["","","","Faible niveau sonore de fonctionnement","dBA","25"]
["","","","Bas","dBA","35"]
["","Rafraîchissement","","Moyen","dBA","40"]
["","","","Faible niveau sonore de fonctionnement","dBA","25"]
["","","","Bas","dBA","35"]
["","","","Haut","dBA","46"]
["Accessoires standard","Manuel d’utilisation","","","","1"]
["","Manuel d'installation","","","","1"]
["","Télécommande infrarouge","","","","1"]
["","Piles sèches AAA","","","","2"]
["","Support de télécommande","","","","1"]
["","Vis de fixation pour plaque de montage","","","","5"]
["","Plaque de montage","","","","1"]
["","Filtre désodorisant à apatite de titane","","","","2"]
["","Vis de fixation du support de la commande à distance","","","","2"]
["","Vis de fixation d'unité intérieure","","","","2"]
["","Cache de vis","","","","2"]
["","Kit d'adaptateur WLAN","","","","1"]
["Systèmes de contrôle","Infrared remote control","","","","ARC466A9"]
["Raccords de tuyauterie","Liquide","","DE","mm","6.35"]
["","Gaz","","DE","mm","12.70"]
["","Évacuation","","","","18"]
["Puissance absorbée","Rafraîchissement","","Nom.","kW","0.033"]
["","Chauffage","","Nom.","kW","0.043"]
["Sound power level","Rafraîchissement","","","dBA","60"]
["","Chauffage","","","dBA","60"]
["Dimensions","Unité","","Largeur","mm","998"]
["","","","Profondeur","mm","212"]
["","","","Hauteur","mm","303"]
["Caisson","Couleur","","","","Argent"]
["Poids","Unité","","","kg","12"]
["Ventilateur","Débit d'air","Chauffage","Haut","m³/min","12.6"]
["","","","Moyen","m³/min","10.5"]
["","","","Bas","m³/min","8.1"]
["","","","Faible niveau sonore de fonctionnement","m³/min","5.0"]
["","","Rafraîchissement","Bas","m³/min","6.8"]
["","","","Moyen","m³/min","8.9"]
["","","","Haut","m³/min","10.9"]
["","","","Faible niveau sonore de fonctionnement","m³/min","3.6"]
["Power supply","Phase","","","","1~"]
["","Nom","","","","V1"]
["","Fréquence","","","Hz","50"]
["","Tension","","","V","220-240"]
["Remarques","","","","","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230 V","(2) - 230 V"]
["","","","","","(3) - 240V","(3) - 240V"]
["Puissance absorbée","Rafraîchissement","","Nom.","kW","","0.023"]
["","Chauffage","","Nom.","kW","","0.031"]
["Caisson","Couleur","","","","","Argent"]
["Dimensions","Unité","","Hauteur","mm","","303"]
["","","","Largeur","mm","","998"]
["","","","Profondeur","mm","","212"]
["Poids","Unité","","","kg","","12"]
["Ventilateur","Débit d'air","Rafraîchissement","Haut","m³/min","","8.9"]
["Ventil.","Débit d'air","Refroidissement","Moyen","m³/min","","6.6"]
["Ventilateur","Débit d'air","Rafraîchissement","Bas","m³/min","","4.4"]
["","","","Faible niveau sonore de fonctionnement","m³/min","","2.6"]
["","","Chauffage","Haut","m³/min","","10.2"]
["Ventil.","Débit d'air","Chauffage","Moyen","m³/min","","8.4"]
["Ventilateur","Débit d'air","Chauffage","Bas","m³/min","","6.3"]
["","","","Faible niveau sonore de fonctionnement","m³/min","","3.8"]
["Niveau de puissance sonore","Rafraîchissement","","","dBA","","54"]
["","Chauffage","","","dBA","","56"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","","38"]
["","Refroidissement","","Moyen","dBA","","32"]
["","","","Bas","dBA","","25"]
["","","","Faible niveau sonore de fonctionnement","dBA","","19"]
["","Chauffage","","Haut","dBA","","40"]
["","","","Moyen","dBA","","34"]
["","","","Bas","dBA","","28"]
["","","","Faible niveau sonore de fonctionnement","dBA","","19"]
["Raccords de tuyauterie","Liquide","","DE","mm","","6.35"]
["","Gaz","","DE","mm","","9.50"]
["","Évacuation","","","","","18"]
["Systèmes de commande","Télécommande infrarouge","","","","","ARC466A9"]
["Accessoires standard","Installation manual","","","","","1"]
["","Wireless remote control","","","","","1"]
["","Screw cover","","","","","2"]
["","AAA dry-cell batteries","","","","","2"]
["","Fixing screw for remote controller holder","","","","","2"]
["","WLAN adapter kit","","","","","1"]
["","Operation manual","","","","","1"]
["","Titanium apatite deodorizing filter","","","","","2"]
["","Fixing screws for mounting plate","","","","","5"]
["","Indoor unit fixing screws","","","","","2"]
["","Mounting plate","","","","","1"]
["","Remote control holder","","","","","1"]
["Alimentation électrique","Nom","","","","","V1"]
["","Phase","","","","","1~"]
["","Fréquence","","","Hz","","50"]
["","Alimentation électrique-=-Tension-=-V","","","V","","220-240"]